Reg.No. \_\_\_\_\_\_\_\_\_\_\_\_



**UNIVERSITY**

(Karunya Institute of Technology & Sciences)

(Declared as Deemed-to-be University under Sec.3 of the UGC Act, 1956)

**Supplementary Examination – June – 2017**

|  |  |  |  |
| --- | --- | --- | --- |
| **Code :** | **14EI2011** | **Duration :** | **3hrs** |
| **Sub. Name :** | **ELECTRONIC INSTRUMENTATION** | **Max. marks :** | **100** |

**ANSWER ALL QUESTIONS (5 x 20 = 100 Marks)**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Q. No | Sub Div. | Questions | Course  Outcome | Marks |
| 1. | a. | Outline the complete circuit of an emitter – follower voltmeter using a FET stage and explain the circuit operation. | CO 1 | 10 |
| b. | Build the block diagram of Vector Impedance meter and explain its operation in detail. | CO 1 | 10 |
| (OR) | | | | |
| 2. | a. | Summarize the block diagram and system waveforms for a DVM using a type analog to digital converter. | CO 1 | 10 |
| b. | Exemplifythe block diagram of Q meter. Explain its operation. | CO 1 | 10 |
| 3. | a. | Construct the basic circuit of an oscilloscope deflection amplifier together with an input attenuator and explain the operation of the circuit. | CO 2 | 14 |
|  | b. | Compare an LED seven segment display with LCD based on the supply current requirement for LED and LCD displays. | CO 2 | 6 |
| (OR) | | | | |
| 4. | a. | Apply ±40V,500Hz triangular to the vertical deflecting plates of a CRT, and a ±50V, 250 Hz sawtooth wave to the horizontal deflecting plates& Examine the waveform in CRT Screen. The CRT has a 0.1 cm/V vertical deflection sensitivity and a 0.08cm/V horizontal deflection sensitivity. Assuming that the two inputs are synchronized. | CO 2 | 14 |
|  | b. | List any four types of displacement transducer & Give one application of each type. | CO 2 | 6 |
| 5. | a. | Explain the function of a sweep frequency generator with neat diagram. | CO 2 | 10 |
|  | b. | Draw a basic block diagram and waveforms for a Digital storage oscilloscope. Sketch the waveforms throughout the system and explain its operation. | CO 2 | 10 |
| (OR) | | | | |
| 6. | a. | Design the logic diagram for a decade counter, and explain its operation. Prepare a table showing the counter output states for each input pulse. | CO 2 | 10 |
|  | b. | Draw the basic block diagram of a digital frequency meter, sketch the waveforms and explain the instrument operation. | CO 2 | 10 |
| 7. | a. | Draftthe Wein’s bridge oscillator circuit diagram.Explain how the circuit operates, and write equations for output frequency and amplifier gain. | CO 2 | 10 |
|  | b. | Summarize the stages involved in engineering of products using virtual instrument with a neat schematic diagram. | CO 3 | 10 |
| (OR) | | | | |
| 8. | a. | Demonstrate the working of function generator to produce various waveform signals with neat sketch. | CO 2 | 10 |
|  | b. | Explain the working principle of spectrum analyzer and describe its working in detail. | CO 2 | 10 |
|  | | **Compulsory**: |  |  |
| 9. | a. | Explain about numeric and Boolean controls and indicators with an example. | CO 3 | 10 |
|  | b. | Explain in detail about the process involved in LabVIEW environment. | CO 3 | 10 |

ALL THE BEST